Cell2Jack Function Description

LED (small)
No light 		: BT is not connected
Red		: BT is connected
Red Slow Flash	: BT is discoverable


LED (big)
Bright Blue		: Power ON and ON-HOOK
Dark Blue		: Power On and OFF-HOOK


Analog Phone DTMF Commands:
     #*#  or 0000		: Enter pairing mode
       *    or 1111		: Enable Siri / Google Talk (Rotary Feature)
    2222XY		: Send XY commands


Option commands ( Enter Keys from your home phone) (red is default)

89#	: Ring back testing
 2#	: Normal LED display
 3#	: Debugging LED display mode
10#	: General Dialing Plan with 10 sec timeout
11#	: General Dialing Plan without timeout
12#   : # only Dialing Plan
14# 	: Enable Call Screening
15#	: Disable Call Screening
18# 	: Enable Rotary Feature
19#	: Disable Rotary Feature
20#	: Regular Ringing strength 
21#	: Strong Ringing strength
24# ~ 28# : Speaker volume level: 0, 1, 2, 3, 4
30# ~ 33# : Hook detection 30, 50, 70, 100 ms
35#	: Enable DTMF Tone Command 
36#	: Disable DTMF Tone Command 
37#	: DTMF threshold Low
38#	: DTMF threshold Normal
39#	: DTMF threshold High
41#	: No dialtone after call disconnect 
42#	: Play dialtone after call disconnect
43#	: Not reverse Tip/Ring after call disconnect
44#	: Reverse Tip/Ring after call disconnect 
50#	: Disable CID
51#	: Enable CID 
60#	: Disable (Media Audio) A2DP streaming 
61#	: Enable (Media Audio) A2DP streaming 
70# ~ 74#	: Off-Hook voltage: High, Medium, Low, Strong, Strongest
82#83#	: Clear Paired device and Reset parameters
80#	: Disable AEC
81#	: Enable AEC 
90# ~ 94# : MIC volume level: 0, 1, 2, 3, 4
99#	: Reboot 


Option Features. (Setting with PC/MAC Application)
    Echo Cancel Depth Control:  Select Echo Depth.
    Rotary Feature: 1111 Enable Siri or Google Voice. 5 seconds to dial independent of calling number length.
    DTMF Input Scaling: Set DTMF detection input scaling value. 


Dual Phone Connection:
1. Press ‘#*#’ to pair first phone.
2. After connected, press ‘#*#’ again to pair second phone.
(Note: Maximum pairing time is 300 seconds.)
3. After connected, both phones will be automatically re-connected once in range. 
(Note:  It will take up to 30 seconds to establish Bluetooth connection)


Hook Flash : Three way talk toggling, answer incoming call during Siri, Call waiting answering.
                       During streaming state, stop the streaming.

Dialing Plan: (Option to enable 5 seconds timeout or only use # to trigger dialing)
10 digits	: 	first digit is not 0 nor 1.
11 digits	: 	first digit is 1 and second digit is not 1.
3 digits	: 	n11 (n = 2 ~ 9)
	>10 digits:	first digit is 0 end with # and length < 20
	<10 digits: 	end with # and length >= 3
	No digit for 10 seconds will trigger the dialing if stored digit number is > 5, 
               Rotary feature is 5 seconds.
	*67 for no-CID outgoing call.

Call Waiting: 
* key or hook flash to answer the new incoming call and hold current call.
* key or hook flash to switch back and forth between calls.
# key to call conference both calls.

